[DLKFET]
Type = NDIS
Title = "D-Link PCI Fast Ethernet Adapter"
Version = 4.39
Drivername = DLKFET$
Xports = NETBEUI LANDD

[FILE]
Name = DLKFET.DOS

; Parameter start

[NETWORKADDRESS]
tag = NETWORKADDRESS
display = "Network adapter address"
type = Hexstring
Strlength = 12
optional = YES
editable = YES
help = "This parameter overrides the network address of the network
 adapter card.  The value of this parameter is a hexadecimal string of
 12 digits, as in 020001020304.  The address
 must be unique among all other network adapter addresses on the
 network."

[SLOT]
tag = SLOT
display = "Slot Number"
type = decimal
range = 1 - 16
optional = YES
editable = YES
help = "This parameter specifies the slot number used for notifications."


[CONNECTIONTYPE]
tag = CONNECTIONTYPE
display = "Connection Type"
type = string
Strlength = 14
Set = AUTOSENSE, _10BASET, _10BASETFD, _100BASETX, _100BASETXFD
default = AUTOSENSE
optional = YES
editable = YES
help = "This parameter specifies the connector type configuration of
 the  network adapter card.  The specification of this parameter depends
 on the specific hardware configuration.  This parameter is used only
 for the D-Link DFE-530TX PCI adapter for Personal Computer AT workstations.
 The parameters are AUTOSENSE, _10BASET, _10BASETFD, _100BASETX,
 and _100BASETXFD."
 
[FLOWCTRL]
tag = FLOWCTRL 
display = "FLOWCTRL "
type = string
Strlength = 16
Set = HARDWARE_DEFAULT, ENABLE, DISABLE
default = HARDWARE_DEFAULT
optional = YES
editable = YES
help = " This keyword is used to specify flow control ability. Driver doesn't care the result of auto-negotiate if 
         the value of this keyword, FLOWCTRL , is ENALBE or DISABLE. It just enables or disable flow control ability
         according your setting."


