   Workstation for DOS ODI Client

   Introduction:
   -------------
   This document describes the procedure to setup the NetWare v3.X , v4.X
   workstation driver for D-Link DFE-538TX 10/100 Adapter.

   Location of Driver:     \NWCLIENT\DOS\DLKRTS.COM

   Sample Configuration Files:
   ---------------------------
     STARTNET.BAT:
        LSL
        DLKRTS
        IPXODI
        NETX or VLM (VLM's for NetWare 4.x )

     NET.CFG:
        LINK DRIVER DLKRTS

        MEDIUM  AUTO     ;operate on auto negotiation mode
;       MEDIUM  10HALF   ;operate on 10M/HalfDuplex mode
;       MEDIUM  10FULL   ;operate on 10M/Fullduplex mode
;       MEDIUM  100HALF  ;operate on 100M/HalfDuplex mode
;       MEDIUM  100FULL  ;operate on 100M/Fullduplex mode

          [ You can use "EtherID" to select a specific DFE-538TX adapter:
           EtherID NNNNNNNNNNNN --Where NNNNNNNNNNNN specify a DFE-538TX
                                  adapter's node address.This is only
                                  required when more than one DFE-538TX
                                  adapters exist on one system.
          ]


           FRAME Ethernet_802.2 --Specify frame type
           FRAME Ethernet_802.3
           FRAME Ethernet_SNAP
           FRAME Ethernet_II

         NetWare DOS Requester
           FIRST NETWORK DRIVE = F
           NETWARE PROTOCOL = NDS BIND
           PREFERRED SERVER = NW411


   Setup Procedures for NetWare 3.11/3.12 Client :
   -----------------------------------------------
      Before you start with the installation process, make sure that
      the adapter is properly installed and configured. Make sure
      that your NetWare workstation is properly installed.

      1. Copy DLKRTS.COM from the D-Link Driver Disk subdirectory
         \NWCLIENT to your harddisk.

      2. Create a batch file, or add to your STARTNET.BAT file the 
         commands listed above under STARTNET.BAT

      3. Edit the NET.CFG file that you copied over. Edit the file per 
         your requirements (see examples above). If there are two frame 
         types listed, whichever frame type is listed first, that is the 
         one that the driver will load. See above for examples.  
         The NET.CFG file should be in the same directory with the 
         LSL.COM file.


   Setup Procedures for NetWare 4.X Client with vlm:
   -------------------------------------------------
      The installation utility INSTALL.EXE is located on NetWare's
      "Workstation for DOS" disk. Run INSTALL.EXE from the Workstation
      for DOS Disk.

      The NetWare Client Install program screen will appear. You must
      complete each of the questions. These options are specific to your
      needs.

      1. Enter the destination directory for the NetWare Client.
         (The default directory is C:\NWCLIENT).

      2. Gives you the option to automatically update the CONFIG.SYS
         and the AUTOEXEC.BAT files or modify them at a later time
         manually.

      3. Do you wish to install support for MS Windows ? (Y/N)
         (MS Windows Subdirectory: default C:\WINDOWS)

      4. Asks you to select a network driver and provide configuration
         options. It uses the specifications you select to create the
         file NET.CFG. Insert the D-Link driver disk when prompted for
         the driver disk and specify the driver path , EX: E:\NWCLIENT\DOS

      5. Press <Enter> to install


   NOTE:
   -----
     1. Be sure to add LASTDRIVE=Z to your CONFIG.SYS file for the
        network mappings to work properly.
     
     2. When you have multiple DFE-538TX Adapters on your system:
        Use "BUSNO" and "DEVICENO" KEYWORD in NET.CFG to select which
        adapter to use with your netware client.(or you can use "EtherID")
