;****************************************************************************
;                                                                
;       Novell NetWare Server Driver Description File for DLKRTS.LAN
;                                                                    
;****************************************************************************

VER: 1.00
SYN: 1.00

DR DLKRTS
{
    DES:    $DLKRTS_1
    HELP:   $DLKRTS_2
    PAR:    2.00
    PROD:   'PCI.10EC.8139.*.*', 'PCI.10EC.8138.*.*', 'PCI.1186.1300.1186.1300.10'

;@# SPROD:  'D-Link~DFE-538TX 10/100 Adapter Driver.'
;@# ALIAS:  DLKRTS.LAN
;@# CLIENT: DLKRTS.LAN

    FILE:   DLKRTS.LAN
    OF:     NBI.NLM, MSM.NLM, ETHERTSM.NLM
    TIME:   15

    PR SLOT
    {
        DES:    $DLKRTS_3
        HELP:   $DLKRTS_4

        TYP:   DEC
        VAL:    1-65535
        DEF:    UND
        OUT:    'SLOT=%s'
    }

    FR FrameSelect
    {
        CD:     $DLKRTS_5
        CH:     $DLKRTS_6
        CD:     $DLKRTS_7
        CH:     $DLKRTS_8
        CD:     $DLKRTS_9
        CH:     $DLKRTS_10
        CD:     $DLKRTS_11
        CH:     $DLKRTS_12
        DEF:    1,2,3,4
    }

    PR NODE OPT
    {
        DES:    $DLKRTS_13
        TYP:   HEX
        VAL:    1-FFFFFFFFFFFE
        DEF:    UND
        OUT:    'NODE=%s'
    }

     PR MEDIUMTYPE   OPT
    {
        DES:    $DLKRTS_14
        HELP:   $DLKRTS_15
        TYP:   STR
        VAL:    AUTO , 100FULL, 100HALF, 10FULL, 10HALF
        DEF:   UND
        OUT:    'MEDIUMTYPE=%s'
    }
}


DLANG:    4
;English
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    6
;French
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    7
;German
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    8
;Italian
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    14
;Spanish
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    12
;Portuquese
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    9
;Japanese
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    10
;Korean
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    1
;Chinese (Simplified)
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    16
;Chinese (Traditional)
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    13
;Russian
    $DLKRTS_1 = "D-Link DFE-538TX 10/100 Adapter Driver."
    $DLKRTS_2 = "This driver supports PCI bus devices"
    $DLKRTS_3 = "Slot"
    $DLKRTS_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $DLKRTS_5 = "802.2"
    $DLKRTS_6 = "ethernet_802.2"
    $DLKRTS_7 = "802.3"
    $DLKRTS_8 = "ethernet_802.3"
    $DLKRTS_9 = "SNAP"
    $DLKRTS_10 = "ethernet_snap"
    $DLKRTS_11 = "ethernet II"
    $DLKRTS_12 = "ethernet_II"
    $DLKRTS_13 = "Node Address"
    $DLKRTS_14 = "MediumType Select"
    $DLKRTS_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"
