;; NETDLKR5.INF (Win2K, WinXP & Win98 combined inf for NDIS5 driver)
;;
;;  D-Link DFE-538TX 10/100 Adapter
;;
;; Copyright 2001-2002, D-Link Corporation. All Rights Reserved.
;;
;; .this release is primarily for motherboard OEM for WHQL test.

[version]
Signature      = "$Chicago$"
Compatible     = 1
Class          = Net
ClassGUID      = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider       = %D-Link%                             ;;
CatalogFile    = NETDLKR5.CAT                               ;; for WHQL certified
CatalogFile.NT = NETDLKRN.CAT
DriverVer      = 08/23/2001,5.397.0823.2001

[Manufacturer]
%D-Link%   = D-Link

[ControlFlags]
;;ExcludeFromSelect     = PCI\VEN_1186&DEV_1300
;;ExcludeFromSelect     = PCI\VEN_1186&DEV_1300&SUBSYS_13001186                 
;;ExcludeFromSelect     = PCI\VEN_10EC&DEV_8139

[D-Link]
%DFE538.DeviceDesc%  = DFE538.ndi, PCI\VEN_1186&DEV_1300
%DFE538_A.DeviceDesc%  = DFE538_A.ndi, PCI\VEN_1186&DEV_1300&SUBSYS_13001186
%DFE538_A.DeviceDesc%  = DFE538_A.ndi, PCI\VEN_10EC&DEV_8139&SUBSYS_13001186

;;****************************************************************************
;; Windows 9x
;;****************************************************************************
[DFE538.ndi]
DriverVer       = 08/23/2001,397
AddReg          = DFE538.id.reg, DFE538.common.reg, DFE538.win.reg, DFE538.oncbs.reg
CopyFiles       = DFE538.CopyFiles98
;DeviceID        = "PCI\VEN_1186&DEV_1300"
;LogConfig       = DefaultConfig

[DFE538_A.ndi]
DriverVer       = 08/23/2001,397
AddReg          = DFE538.id.reg, DFE538.common.reg, DFE538.win.reg, DFE538.oncbs.reg
CopyFiles       = DFE538.CopyFiles98
;DeviceID        = "PCI\VEN_1186&DEV_1300&SUBSYS_13001186"
;LogConfig       = DefaultConfig

;;****************************************************************************
;; Win2K, WinXP
;;****************************************************************************
[DFE538.ndi.NT]
AddReg          = DFE538.common.reg, DFE538.reg, DFE538.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = DFE538.CopyFiles

[DFE538.ndi.NT.Services]
AddService = DLKRTS, 2, rtsnt.Service, DFE538.EventLog

[DFE538_A.ndi.NT]
AddReg          = DFE538.common.reg, DFE538.reg, DFE538.oncbs.reg
Characteristics = 0x84
BusType         = 5
CopyFiles       = DFE538.CopyFiles

[DFE538_A.ndi.NT.Services]
AddService = DLKRTS, 2, rtsnt.Service, DFE538.EventLog

[DFE538.CopyFiles]
DLKRTS.SYS,,,2

[DFE538.CopyFiles98]
DLKRTS.SYS,,,2

;;----------------------------------------------------------------------------
;; DFE-538TX Parameters
;;----------------------------------------------------------------------------
;;***************************************************************************
;; Windows 9x parameters
;;***************************************************************************
[DFE538.id.reg]
HKR, Ndi,       DeviceID,       0,      "PCI\VEN_1186&DEV_1300"

HKR, Ndi\Install,                       ,       0,      rtsnt.install
HKR, NDI\Params\DuplexMode,             flag,   1,      30, 00, 00, 00
HKR, Ndi\Params\EarlyTxThreshold,       flag,   1,      20, 00, 00, 00
HKR, NDI\Params\NetworkAddress,         flag,   1,      30, 00, 00, 00
HKR, NDI\Params\WakeUpFrame,            flag,   1,      30, 00, 00, 00

[DFE538.win.reg]
;; key,subkey,valuname,type,value
HKR, ,  DriverDesc,     0,      "D-Link DFE-538TX 10/100 Adapter"
HKR, ,  DevLoader,      0,      *ndis
HKR, ,  DeviceVxDs,     0,      DLKRTS.SYS
HKR, ,  EnumPropPages,  0,      netdi.dll,      EnumPropPages

;;params
HKR, ,  MediaType,      0,      1
HKR, ,  AdapterType,    0,      5
HKR, ,  BusType,        0,      5

;; NDIS Info
HKR, NDIS,              MajorNdisVersion,       1,      03
HKR, NDIS,              MinorNdisVersion,       1,      0a
HKR, NDIS,              LogDriverName,          0,      "DLKRTS"

;; Interfaces
HKR, Ndi\Interfaces,    DefLower,               ,       "ethernet"
HKR, Ndi\Interfaces,    LowerRange,             ,       "ethernet"
HKR, Ndi\Interfaces,    DefUpper,               ,       "ndis3"
HKR, Ndi\Interfaces,    UpperRange,             ,       "ndis3"

;; Install sections
HKR, Ndi\Install,       ndis3,                  0,      "DFE538.ndis5"

;;****************************************************************************
;; DFE-538TX common parameters
;;****************************************************************************
[DFE538.oncbs.reg]
HKR,,ChipOnCardbus,,"0"

[DFE538.common.reg]
HKR, Ndi\params\DuplexMode,      ParamDesc, 0, %DuplexMode%
HKR, Ndi\params\DuplexMode,      type,      0, "enum"
HKR, Ndi\params\DuplexMode,      default,   0, "1"
HKR, Ndi\params\DuplexMode\enum, 1,         0, %dmAutoMode%
HKR, Ndi\params\DuplexMode\enum, 2,         0, %dm10HalfMode%
HKR, Ndi\params\DuplexMode\enum, 3,         0, %dm10FullMode%
HKR, Ndi\params\DuplexMode\enum, 4,         0, %dm100HalfMode%
HKR, Ndi\params\DuplexMode\enum, 5,         0, %dm100FullMode%

HKR,Ndi\Params\EarlyTxThreshold, ParamDesc, 0, %EarlyTxThreshold%
HKR,Ndi\Params\EarlyTxThreshold, Type,      0, "int"
HKR,Ndi\Params\EarlyTxThreshold, Default,   0, "15"
HKR,Ndi\Params\EarlyTxThreshold, Min,       0, "0"
HKR,Ndi\Params\EarlyTxThreshold, Max,       0, "63"
HKR,Ndi\Params\EarlyTxThreshold, Step,      0, "1"
HKR,Ndi\Params\EarlyTxThreshold, Base,      0, "10"

HKR,Ndi\params\NetworkAddress,   ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,   type,      0, "edit"
HKR,Ndi\params\NetworkAddress,   default,   0, "000000000000"
HKR,Ndi\params\NetworkAddress,   LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress,   UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress,   Optional,  0, "1"

;HKR,NDI\Params\TxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\TxMaxDMABurst,ParamDesc,0,"Transmit DMA burst size"
;HKR,Ndi\params\TxMaxDMABurst,type,0,enum
;HKR,Ndi\params\TxMaxDMABurst,default,0,6
;HKR,Ndi\params\TxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\TxMaxDMABurst\enum,7,0,"7:2048 bytes"

;HKR,NDI\Params\RxMaxDMABurst,flag,1,30,00,00,00
;HKR,Ndi\params\RxMaxDMABurst,ParamDesc,0,"Receive DMA burst size"
;HKR,Ndi\params\RxMaxDMABurst,type,0,enum
;HKR,Ndi\params\RxMaxDMABurst,default,0,6
;HKR,Ndi\params\RxMaxDMABurst\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\RxMaxDMABurst\enum,7,0,"7:unlimitted"

;HKR,NDI\Params\EarlyRxThreshold,flag,1,30,00,00,00
;HKR,Ndi\params\EarlyRxThreshold,ParamDesc,0,"Receive FIFO threshold"
;HKR,Ndi\params\EarlyRxThreshold,type,0,enum
;HKR,Ndi\params\EarlyRxThreshold,default,0,2
;HKR,Ndi\params\EarlyRxThreshold\enum,0,0,"0:16 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,1,0,"1:32 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,2,0,"2:64 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,3,0,"3:128 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,4,0,"4:256 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,5,0,"5:512 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,6,0,"6:1024 bytes"
;HKR,Ndi\params\EarlyRxThreshold\enum,7,0,"7:No threshold"

;HKR,NDI\Params\TxInterFrameGap,flag,1,30,00,00,00
;HKR,Ndi\params\TxInterFrameGap,ParamDesc,0,"Tx IFG(10M/100M)"
;HKR,Ndi\params\TxInterFrameGap,type,0,enum
;HKR,Ndi\params\TxInterFrameGap,default,0,3
;HKR,Ndi\params\TxInterFrameGap\enum,0,0,"8.4us/840ns"
;HKR,Ndi\params\TxInterFrameGap\enum,1,0,"8.8us/880ns"
;HKR,Ndi\params\TxInterFrameGap\enum,2,0,"9.2us/920ns"
;HKR,Ndi\params\TxInterFrameGap\enum,3,0,"9.6us/960ns"

;HKR, Ndi\params\WakeOnLan,         ParamDesc,  0, "Smart Power Saving"
;HKR, Ndi\params\WakeOnLan,         default,    0, "0"  
;HKR, Ndi\params\WakeOnLan,         type,       0, "enum"
;HKR, Ndi\params\WakeOnLan\enum,    "0",        0, "Disable"
;HKR, Ndi\params\WakeOnLan\enum,    "1",        0, "Enable (No WakeUp)"

HKR,Ndi\params\RxBufLen,	   ParamDesc,  0, "Receive Buffer Size"
HKR,Ndi\params\RxBufLen,	   type,       0, "enum"
HKR,Ndi\params\RxBufLen,	   default,    0, "3"
HKR,Ndi\params\RxBufLen\enum,	   "0",	       0, "8K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "1",	       0, "16K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "2",	       0, "32K bytes"
HKR,Ndi\params\RxBufLen\enum,	   "3",	       0, "64K bytes"

HKR, Ndi\params\LinkUp,            ParamDesc,  0, "WakeUp on Link Change"
HKR, Ndi\params\LinkUp,            default,    0, "0"
HKR, Ndi\params\LinkUp,            type,       0, "enum"
HKR, Ndi\params\LinkUp\enum,       "1",        0, "Enable"
HKR, Ndi\params\LinkUp\enum,       "0",        0, "Disable"

HKR, Ndi\params\WakeUpFrame,       ParamDesc,  0, "WakeUp on ARP/PING"
HKR, Ndi\params\WakeUpFrame,       default,    0, "0"
HKR, Ndi\params\WakeUpFrame,       type,       0, "enum"
HKR, Ndi\params\WakeUpFrame\enum,  "0",        0, "Enable"
HKR, Ndi\params\WakeUpFrame\enum,  "1",        0, "Disable"

HKR, Ndi\params\PME,               ParamDesc,  0, "WakeUp using APM Mode"
HKR, Ndi\params\PME,               default,    0, "1"
HKR, Ndi\params\PME,               type,       0, "enum"
HKR, Ndi\params\PME\enum,          "0",        0, "Enable"
HKR, Ndi\params\PME\enum,          "1",        0, "Disable"

HKR, Ndi\params\EnableLDPS,        ParamDesc,  0, "Link Down Power Saving"
HKR, Ndi\params\EnableLDPS,        default,    0, "0"
HKR, Ndi\params\EnableLDPS,        type,       0, "enum"
HKR, Ndi\params\EnableLDPS\enum,   "0",        0, "Disable"
HKR, Ndi\params\EnableLDPS\enum,   "1",        0, "Enable"


;;****************************************************************************
;; Win2K, WinXP parameters
;;****************************************************************************
[DFE538.reg]
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"
HKR, Ndi,                       Service,    0, "DLKRTS"

[rtsnt.Service]
DisplayName     = %DFE538.Service.DispName%
ServiceType     = 1                             ; %SERVICE_KERNEL_DRIVER%
StartType       = 3                             ; %SERVICE_DEMAND_START%
ErrorControl    = 1                             ; %SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\DLKRTS.SYS
LoadOrderGroup  = NDIS

[DFE538.EventLog]
Addreg = DFE538.AddEventLog.reg

[DFE538.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,    ,   TypesSupported,     0x00010001, 7

;;****************************************************************************
;; Destination Directory
;;****************************************************************************
[DestinationDirs]
DFE538.CopyFiles           = 12
DFE538.CopyFiles98         = 11
DefaultDestDir              = 11        ; LDID_SYS

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksNames]
1=%DISKNAME%,,,

[SourceDisksFiles]
DLKRTS.SYS  = 1
DLKRTS.SYS  = 1              ;;Windows 2K,XP 
;NETDLKR5.INF  = 1
;NETDLKR5.INF  = 1             ;;Windows 2K,XP
;NETDLKR5.CAT  = 1
;NETDLKRN.CAT  = 1

;;****************************************************************************
;; Strings
;;****************************************************************************
[Strings]
;Msft                      = "D-Link Corporation."
D-Link                   = "D-Link Corporation."

;;Source disk name
DISKNAME = "D-Link DFE-538TX 10/100 Adapter Driver Disk"

NetworkAddress            = "Network Address"
EarlyTxThreshold          = "Early Tx Threshold"
DuplexMode                = "Link Speed/Duplex Mode"
dmAutoMode                = "Auto Mode"
dm10HalfMode              = "10 Half Mode"
dm10FullMode              = "10 Full Mode"
dm100HalfMode             = "100 Half Mode"
dm100FullMode             = "100 Full Mode"

DFE538.DeviceDesc        = "D-Link DFE-538TX 10/100 Adapter"
DFE538.Service.DispName  = "D-Link DFE-538TX 10/100 Adapter"
DFE538_A.DeviceDesc      = "D-Link DFE-538TX 10/100 Adapter"
