;****************************************************************************************
;
; Dnetr28ux.inf
;
;   This installation script supports Windows Vista, Win7 for the
;   D-Link series USB Wireless LAN Card.
;
;   Copyright (c)2002-2009 , D-Link Corp., All Rights Reserved.
;
;**************************************************************************************

[Version]
Signature       = "$Windows NT$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Provider%
CatalogFile     = Dnetr28ux.cat ; For WHQL certification.
DriverVer       = 08/05/2009, 3.00.03.0000

[ControlFlags]
;***********D-Link 802.11n board  ***********
ExcludeFromSelect = *

[Manufacturer]
%D-Link%        = D-Link, NTAMD64.6.1


;*******************************************************************************************
; Win7 specific entries
;*******************************************************************************************
[D-Link.NTAMD64.6.1]
; DisplayName                   Section                     DeviceID
; -----------                   -------                     --------
%DWA-140B1_3C09.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C09
%DWA-160B1_3C11.DeviceDesc%    = OS61_RTWLANH_C2.ndi,        USB\VID_07D1&PID_3C11
%DWA-130B1_3C13.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C13
%DWA-140B2_3C0A.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C0A
%DWA-110B1_3C0B.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C0B
%DWA-125A1_3C0D.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C0D
%WUA-2340B1_3C0E.DeviceDesc%   = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C0E
%DWL-G122E1_3C0F.DeviceDesc%   = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C0F
%DWA-140B3_3C15.DeviceDesc%    = OS61_RTWLAN_C2.ndi,         USB\VID_07D1&PID_3C15


;*******************************************************************************************
; Win7 specific entries
;*******************************************************************************************

[OS61_RTWLAN.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANR.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANDR.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, SingleBand.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ;USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANRG.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANRGL.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, SingleBand.reg, AdhocN.reg, RemoveFlag.reg, LinkSpeedStatus.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANHC.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg, CarrierDetect.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANS.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, SmartScan.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANR_Az.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, RemoveFlag.reg, CoInstOpt_DisableN.reg, LinkSpeedStatus.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLAN_Abo.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, InitChn14Disabled.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLAN_C1.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, Customer1.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLAN_C2.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, Customer2.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANH_C2.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, IEEE80211H.reg, Customer2.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

[OS61_RTWLANR_C3.ndi.NT]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
AddReg                  = Common.reg, RTUSB_OS61.ndi.NT.reg, DefaultBand.reg, AdhocN.reg, RemoveFlag.reg, CoInstOpt_DisableN.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 15                        ; USB
CopyFiles               = NT.CopyFiles
*IfType = 71              ; IF_TYPE_IEEE80211
*MediaType = 16           ; NdisMediumNative802_11
*PhysicalMediaType = 9    ; NdisPhysicalMediumNative802_11

;*******************************************************************************************
; Win7 services sections
;*******************************************************************************************
[OS61_RTWLAN.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLAN.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANR.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANR.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANDR.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANDR.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANRG.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANRG.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANRGL.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANRGL.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANHC.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANHC.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANS.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANS.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANR_Az.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANR_Az.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLAN_Abo.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLAN_Abo.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLAN_C1.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLAN_C1.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLAN_C2.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLAN_C2.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANH_C2.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANH_C2.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

[OS61_RTWLANR_C3.ndi.NT.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService              = netr28ux, 2, Generic.Service, common.EventLog

[OS61_RTWLANR_C3.ndi.NT.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration

;*******************************************************************************************
; NT CoInstallers Sections
;*******************************************************************************************
[OS61_RTWLAN.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANR.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANDR.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANRG.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANRGL.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANHC.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANS.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANR_Az.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLAN_Abo.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLAN_C1.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLAN_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANH_C2.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

[OS61_RTWLANR_C3.ndi.NT.CoInstallers]
CopyFiles = CoInstaller.CopyFiles
AddReg = CoInstaller_AddReg

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "5"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "1"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Disable 5GHz adhoc mode
;
HKR, ,                            Adhoc5GDisable,  0, "0"

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
;HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
;HKR, NDI\params\Radio,            type,            0, "enum"
;HKR, NDI\params\Radio,            default,         0, "0"
;HKR, NDI\params\Radio\enum,       1,               0, %Disable%
;HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%

;
; RDG
;
HKR, ,                            RDG,      0, "1"

;
; Power Saving Control
;
HKR, ,                            PSControl,       0x00010001, 0x00000000

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "1"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, %WMMCapable%
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "1"
HKR, NDI\params\WMMCapable\enum,        0,         0, %Disable%
HKR, NDI\params\WMMCapable\enum,        1,         0, %Enable%

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
;HKR, NDI\params\APSDCapable,            ParamDesc, 0, %APSDCapable%
;HKR, NDI\params\APSDCapable,            type,      0, "enum"
;HKR, NDI\params\APSDCapable,            default,   0, "1"
;HKR, NDI\params\APSDCapable\enum,       0,         0, %Disable%
;HKR, NDI\params\APSDCapable\enum,       1,         0, %Enable%

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
;HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, %APSDAC_BE%
;HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
;HKR, NDI\params\APSDAC_BE,              default,   0, "1"
;HKR, NDI\params\APSDAC_BE\enum,         0,         0, %Disable%
;HKR, NDI\params\APSDAC_BE\enum,         1,         0, %Enable%

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
;HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, %APSDAC_BK%
;HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
;HKR, NDI\params\APSDAC_BK,              default,   0, "1"
;HKR, NDI\params\APSDAC_BK\enum,         0,         0, %Disable%
;HKR, NDI\params\APSDAC_BK\enum,         1,         0, %Enable%

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
;HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, %APSDAC_VI%
;HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
;HKR, NDI\params\APSDAC_VI,              default,   0, "1"
;HKR, NDI\params\APSDAC_VI\enum,         0,         0, %Disable%
;HKR, NDI\params\APSDAC_VI\enum,         1,         0, %Enable%

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
;HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, %APSDAC_VO%
;HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
;HKR, NDI\params\APSDAC_VO,              default,   0, "1"
;HKR, NDI\params\APSDAC_VO\enum,         0,         0, %Disable%
;HKR, NDI\params\APSDAC_VO\enum,         1,         0, %Enable%

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
;HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
;HKR, NDI\params\IEEE80211H,       type,            0, "enum"
;HKR, NDI\params\IEEE80211H,       default,         0, "0"
;HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
;HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "1"
HKR, NDI\params\SmartScan,        ParamDesc,       0, %SmartScan%
HKR, NDI\params\SmartScan,        type,            0, "enum"
HKR, NDI\params\SmartScan,        default,         0, "0"
HKR, NDI\params\SmartScan\enum,   0,               0, %Disable%
HKR, NDI\params\SmartScan\enum,   1,               0, %Enable%

;
; Block ACK settings
;
HKR, ,                            BACapability,      0x10001, "0x07034040"
HKR, Default,                     BACapability,      0x10001, "0x07034040"

;
; Transmit Rate setting
;
HKR, ,                            TransmitSetting,      0x10001, "0x2ba15"
HKR, Default,                     TransmitSetting,      0x10001, "0x2ba15"

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;
; ProhibitTKIPonHT
;
HKR, ,                            ProhibitTKIPonHT,   0, "1"

;
; Link Speed Status
;
HKR, ,                            LinkSpeedStatus, 0, "0"

[RemoveFlag.reg]
HKR, ,                SafelyRemoveOff,    0, "1"

[IEEE80211H.reg]
HKR, ,                IEEE80211H,         0, "1"

[CarrierDetect.reg]
HKR, ,                CarrierDetect,      0, "1"

[SmartScan.reg]
HKR, ,                SmartScan,          0, "1"

[AdhocN.reg]
;
; AdhocNMode
;
HKR, ,                            AdhocNMode,      0, "0"
;HKR, NDI\params\AdhocNMode,       ParamDesc,       0, %AdhocNMode%
;HKR, NDI\params\AdhocNMode,       type,            0, "enum"
;HKR, NDI\params\AdhocNMode,       default,         0, "0"
;HKR, NDI\params\AdhocNMode\enum,  0,               0, %Disable%
;HKR, NDI\params\AdhocNMode\enum,  1,               0, %Enable%

; Disable Channel 14 for JP
[InitChn14Disabled.reg]
HKR, ,                    InitChn14Disabled,      0,"1"

[SingleBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
;HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
;HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
;HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
;HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
;HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
;HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
;HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

[DefaultBand.reg]
;
; 2.4G Band
;
HKR, ,                                 CountryRegion,      0, "0"
;HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
;HKR, NDI\params\CountryRegion,         type,               0, "enum"
;HKR, NDI\params\CountryRegion,         default,            0, "0"
;HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
;HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
;HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
;HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
;HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
;HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
;HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
;HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; 5G Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
;HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
;HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
;HKR, NDI\params\CountryRegionABand,    default,            0, "0"
;HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
;HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
;HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
;HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
;HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
;HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
;HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
;HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
;HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
;HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
;HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%
;HKR, NDI\params\CountryRegionABand\enum,11,                0, %CountryRegion5G_11%
;HKR, NDI\params\CountryRegionABand\enum,12,                0, %CountryRegion5G_12%
;HKR, NDI\params\CountryRegionABand\enum,13,                0, %CountryRegion5G_13%
;HKR, NDI\params\CountryRegionABand\enum,14,                0, %CountryRegion5G_14%
;HKR, NDI\params\CountryRegionABand\enum,15,                0, %CountryRegion5G_15%
;HKR, NDI\params\CountryRegionABand\enum,16,                0, %CountryRegion5G_16%

;
; Customer Request
;

; Customer request for Corega2
[Customer1.reg]
; WPS Device Name
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%

[Customer2.reg]
;
; D-Link Request
;
; WMMCapable
HKR, ,                            WMMCapable,      0, "1"
; Show Hidden SSID in Site Survey Page
HKR, ,                            ShowHiddenSSID,  0, "1"   ; 0=disable(default), 1=enable
; Enable TX Burst
HKR, ,                            TXBurst,         0, "1"
; FrameAggregation
HKR, ,                            FrameAggregation,0, "1"
; DLSCapable
HKR, ,                            DLSCapable,      0, "1"

[LinkSpeedStatus.reg]
;
; LinkSpeedStatus
;
HKR, ,                            LinkSpeedStatus, 0, "1"

;
; RaCoInstaller Options
; CoInstaller Options , Enable 11n feature in Morocco, Russia, Ukraine.
[CoInstOpt_DLink.reg]
HKR, ,                            RaCoInstOpt,      0,"00001111"
; WirelessMode
HKR, ,                            WirelessMode,    0, "5"
; CountryWirelessMode
HKR, ,                            CountryWirelessMode,    0x10001, "0x11101110"

; CoInstaller Option for Aurewave, MSI
[CoInstOpt_DisableN.reg]
HKR, ,                    RaCoInstOpt,      0,"00001111"

; WirelessMode
HKR, ,                            WirelessMode,    0, "3"

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "RaCoInstx.dll,ClassCoInstaller"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************
[NT.CopyFiles]
Dnetr28ux.sys,,,2

[CoInstaller.CopyFiles]
RaCoInstx.dll,,,2
RaCoInst.dat,,,2

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
Dnetr28ux.sys              = 1,,
RaCoInstx.dll              = 1,,
RaCoInst.dat               = 1,,

[DestinationDirs]
NT.CopyFiles     = 12     ; system32\drivers subdirectory on NT
DefaultDestDir   = 11
CoInstaller.CopyFiles	= 11

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RTUSB_OS61.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "netr28ux"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "wlan,ethernet,vwifi"

[Generic.Service]
DisplayName                 = %Generic.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\Dnetr28ux.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\Dnetr28ux.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "D-Link Corporation"
D-Link                      = "D-Link Corporation"
DWA-140B1_3C09.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter"
DWA-160B1_3C11.DeviceDesc      = "D-Link DWA-160 Xtreme N Dual Band USB Adapter(rev.B)"
DWA-130B1_3C13.DeviceDesc      = "D-Link DWA-130 Wireless N USB Adapter(rev.B)"
DWA-140B2_3C0A.DeviceDesc      = "D-Link DWA-140 RangeBooster N USB Adapter(rev.B2)"
DWA-110B1_3C0B.DeviceDesc      = "D-Link DWA-110 Wireless G USB Adapter(rev.B)"
DWA-125A1_3C0D.DeviceDesc      = "D-Link DWA-125 Wireless 150 USB Adapter"
WUA-2340B1_3C0E.DeviceDesc     = "D-Link WUA-2340 USB Adapter(rev.B)"
DWL-G122E1_3C0F.DeviceDesc     = "D-Link AirPlus G DWL-G122 Wireless Adapter(rev.E)"
DWA-140B3_3C15.DeviceDesc      = "D-Link DWA-140 Wireless N USB Adapter(rev.B3)"

INSTALL_DISK_STR            = "D-Link dnetr28u Wireless 11n USB Installation Disk"
Generic.Service.DispName    = "D-Link dnetr28u USB Extensible Wireless LAN Card Driver"

;
; Parameters
;
RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
AdhocNMode                  = "Adhoc support 802.11n"

CHANNEL                     = "6"
WPS_DEVNAME_DEF_STR         = "D-Link Client"
WPS_DEVNAME_CUSTOMER1       = "D-Link Client"
WMMCapable                  = "WMM Capable"
APSDCapable                 = "APSD Capable"
APSDAC_BE                   = "AC_BE support APSD"
APSDAC_BK                   = "AC_BK support APSD"
APSDAC_VI                   = "AC_VI support APSD"
APSDAC_VO                   = "AC_VO support APSD"
