;/*++
;
;Copyright (c) 2004 D-Link Corporation, Incorporated All Rights Reserved
;
;Module Name:
;
;    netA3AB.inf

;
;Abstract:
;    For US
;    INF file for installing D-Link 802.11a/b/g Wireless Adapter
; 
;    Installs A3AB.sys (NDIS 5/5.1 driver) on NT platforms (2000, XP and greater)
;    Installs A3AB9x.sys (NDIS 5 driver) on 9x platforms 

;--*/

[Version]
Signature   = "$CHICAGO$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %DLink%
Compatible  = 1
DriverVer   = 03/28/2005,3.3.2.16
;Catalogfile = A3AB.cat

[Manufacturer]
%DLink%     = DLink

[ControlFlags]
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A121186
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A131186
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A141186
ExcludeFromSelect = VEN_168C&DEV_001A&SUBSYS_3A151186
ExcludeFromSelect = VEN_168C&DEV_001A&SUBSYS_3A161186
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A171186
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A181186
ExcludeFromSelect = VEN_168C&DEV_0013&SUBSYS_3A631186
ExcludeFromSelect = VEN_168C&DEV_001B&SUBSYS_3A191186
ExcludeFromSelect = VEN_168C&DEV_001B&SUBSYS_3A221186
ExcludeFromSelect = VEN_168C&DEV_001A&SUBSYS_3A231186
ExcludeFromSelect = VEN_168C&DEV_001A&SUBSYS_3A241186

[DLink]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------

%G650.DeviceDesc%   = G650_SEC.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%G520.DeviceDesc%   = G520_SEC.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%AG530.DeviceDesc%  = AG530_SEC.ndi, 	PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%G630.DeviceDesc%   = G630_SEC.ndi,	PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%G510.DeviceDesc%   = G510_SEC.ndi,	PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%AG660.DeviceDesc%  = AG660_SEC.ndi, 	PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%G680.DeviceDesc%   = G680_SEC.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%G550.DeviceDesc%   = G550_SEC.ndi,	PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%AG660B.DeviceDesc%  = AG660B_SEC.ndi, 	PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%AG530B.DeviceDesc%  = AG530B_SEC.ndi, 	PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%G650P.DeviceDesc%   = G650P_SEC.ndi,	PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%G520P.DeviceDesc%   = G520P_SEC.ndi,	PCI\VEN_168C&DEV_001A&SUBSYS_3A231186

; Windows 9X specific entries
[G650_SEC.ndi]
AddReg          = G650_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.sbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G680_SEC.ndi]
AddReg          = G680_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.sbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G630_SEC.ndi]
AddReg          = G630_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.bg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G650P_SEC.ndi]
AddReg          = G650P_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.bg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G520_SEC.ndi]
AddReg          = G520_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.psbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G550_SEC.ndi]
AddReg          = G550_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.psbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G510_SEC.ndi]
AddReg          = G510_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.pbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G520P_SEC.ndi]
AddReg          = G520P_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.pbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG530_SEC.ndi]
AddReg          = AG530_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.psabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG660_SEC.ndi]
AddReg          = AG660_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.sabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG660B_SEC.ndi]
AddReg          = AG660B_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.sabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG530B_SEC.ndi]
AddReg          = AG530B_SEC.id.reg, 5211.reg, A3AB.win.reg, 5212.psabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.win.CopyFiles, Ndi_9X_CopyFiles, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

; Windows NT specific entry

[G650_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.sbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G680_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.sbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G630_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.bg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G650P_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.bg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G520_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.psbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G550_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.psbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G510_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.pbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G520P_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.pbg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG530_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.psabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG660_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.sabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG660B_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.sabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[AG530B_SEC.ndi.NT]
Characteristics = 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType         = 5
AddReg          = A3AB.reg, 5211.reg, 5212.psabg.reg
DelReg		= 5211.DelReg
CopyFiles       = A3AB.CopyFiles.nt, DEFAULTDESTDIRS
DelFiles        = A3AB.DelIniFiles

[G650_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G650_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G680_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G680_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G630_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G630_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G650P_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G650P_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G520_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G520_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G520P_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G520P_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G550_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G550_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[G510_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[G510_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[AG530_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[AG530_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[AG660_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[AG660_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[AG660B_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[AG660B_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[AG530B_SEC.ndi.NT.Services]
AddService      = A3AB, 2, A3AB.Service, common.EventLog
[AG660B_SEC.ndi.NT.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles


[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"DWLInst.dll,DWLInst"

						
;----------------------------------------------------------------------------
; Win9x id registry sections
; These are not needed by NT

[G650_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A121186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G680_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A171186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G630_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_3A151186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G650P_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_3A241186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G520_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A131186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G550_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A181186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G510_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_3A161186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[G520P_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001A&SUBSYS_3A231186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[AG530_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A141186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[AG660_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0013&SUBSYS_3A631186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[AG660B_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_3A191186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

[AG530B_SEC.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_001B&SUBSYS_3A221186"
HKR, Ndi, NdiInstaller, 0, "DWLNdi.dll, DWLNDIProc"

; 5212 Enumerated Types
;
[5212.sbg.reg]
HKR, ,			NetBand,		0x00002,  "28"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,			NicType,		0x10003,  "0"
HKR, ,			p24GAG,			0x00002,  "0"
HKR, ,			p5GAG,			0x00002,  "2"
HKR, ,			abolt,			0x00002,  "255"
HKR, ,			WmmEnabled,		0x00002,  "0"

[5212.psbg.reg]
HKR, ,			NetBand,		0x00002,  "28"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,       		NicType,		0x10003,  "0"
HKR, ,			p24GAG,			0x00002,  "2"
HKR, ,			p5GAG,			0x00002,  "4"
HKR, ,			abolt,			0x00002,  "255"
HKR, ,			WmmEnabled,		0x00002,  "0"

[5212.pbg.reg]
HKR, ,			NetBand,		0x00002,  "12"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,       		NicType,		0x10003,  "0"
HKR, ,			p24GAG,			0x00002,  "2"
HKR, ,			p5GAG,			0x00002,  "4"
HKR, ,			abolt,			0x00002,  "0"
HKR, ,			WmmEnabled,		0x00002,  "0"
HKR, ,			AuthWPA2,		0x00002,  "0"

[5212.bg.reg]
HKR, ,			NetBand,		0x00002,  "12"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,       		NicType,		0x10003,  "0"
HKR, ,			p24GAG,			0x00002,  "0"
HKR, ,			p5GAG,			0x00002,  "2"
HKR, ,			abolt,			0x00002,  "0"
HKR, ,			WmmEnabled,		0x00002,  "0"
HKR, ,			AuthWPA2,		0x00002,  "0"

[5212.sabg.reg]
HKR, ,			NetBand,		0x00002,  "31"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,       		NicType,		0x10003,  "1"
HKR, ,			p24GAG,			0x00002,  "0"
HKR, ,			p5GAG,			0x00002,  "2"
HKR, ,			abolt,			0x00002,  "255"

[5212.psabg.reg]
HKR, ,			NetBand,		0x00002,  "31"
HKR, ,			AdHocBand,		0x00002,  "0"
HKR, ,       		NicType,		0x10003,  "2"
HKR, ,			p24GAG,			0x00002,  "2"
HKR, ,			p5GAG,			0x00002,  "4"
HKR, ,			abolt,			0x00002,  "255"

;-----------------------------------------------------------------------------


[5211.reg.security]
"D:ARAI(A;;GA;;;BA)(A;;GA;;;SY)(A;CI;GA;;;IU)"

;
; 5211 common
;
[5211.DelReg]
HKR, ,abolt


[5211.reg]

HKR, Ndi\params\MapRegisters,		ParamDesc,	0,  %MapRegisters%
HKR, Ndi\params\MapRegisters,		default,	0,  "256"
HKR, Ndi\params\MapRegisters,		min,		0,  "32"
HKR, Ndi\params\MapRegisters,		max,		0,  "512"
HKR, Ndi\params\MapRegisters,		step,		0,  "8"
HKR, Ndi\params\MapRegisters,		base,		0,  "10"
HKR, Ndi\params\MapRegisters,		type,		0,  "int"

HKR, Ndi\params\NetworkAddress,		ParamDesc,	0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,		default,	0,  ""
HKR, Ndi\params\NetworkAddress,		LimitText,	0,  "12"
HKR, Ndi\params\NetworkAddress,		UpperCase,	0,  "1"
HKR, Ndi\params\NetworkAddress,		optional,	0,  "1"
HKR, Ndi\params\NetworkAddress,		type,		0,  "edit"


HKR, Ndi\params\sleepMode,		ParamDesc,	0,  %sleepMode%
HKR, Ndi\params\sleepMode,		Base,		0,  "10"
HKR, Ndi\params\sleepMode,		default,	0,  "0"
HKR, Ndi\params\sleepMode,		type,		0,  "enum"
HKR, Ndi\params\sleepMode\enum,		"0",		0,  %sleepModeOff%
HKR, Ndi\params\sleepMode\enum,		"2",		0,  %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum,		"1",		0,  %sleepModeMax%

HKR, Ndi\params\tpc,                    ParamDesc,                      0,  %tpc%
HKR, Ndi\params\tpc,                    Base,                           0,  "10"
HKR, Ndi\params\tpc,                    default,                        0,  "0"
HKR, Ndi\params\tpc,                    type,                           0,  "enum"
HKR, Ndi\params\tpc\enum,               "0",                            0,  %tpc100%
HKR, Ndi\params\tpc\enum,               "1",                            0,  %tpc50%
HKR, Ndi\params\tpc\enum,               "2",                            0,  %tpc25%
HKR, Ndi\params\tpc\enum,               "3",                            0,  %tpc12%
HKR, Ndi\params\tpc\enum,               "4",                            0,  %tpcLowest%

HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,  "10"
HKR, Ndi\params\shortPreamble,          default,                        0,  "1"
HKR, Ndi\params\shortPreamble,          type,                           0,  "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,  %shortPreambleDisable%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,  %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,  "10"
HKR, Ndi\params\radioEnable,            default,                        0,  "1"
HKR, Ndi\params\radioEnable,            type,                           0,  "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,  %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,  %radioEnableOff%

HKR, ,		         		pciDetectEnable,			0x00002,  "1"
HKR, ,		         		BusType,			0x00002,  "5"
HKR, ,			AdHocChannel,			0x00002,  "2437"
;HKR, ,                                  AdHocBand,                      0x00002,  "0"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"
HKR, ,                                  beaconInterval,                 0x00002,  "100"
HKR, ,                                  bkScanEnable,                   0x00002,  "1"
HKR, ,                                  bssType,                        0x00002,  "1"
HKR, ,                                  ccode,                          0x00002,  "US"
HKR, ,                                  clist,                          0x00002,  ""
HKR, ,                                  defaultKey,                     0x00002,  "0"
HKR, ,                                  EncryptionAlg,                  0x00002,  "2"
HKR, ,                                  FragThreshold,                  0x00002,  "2346"
HKR, ,                                  HwTxRetries,                    0x00002,  "4"
HKR, ,                                  privacyInvoked,                 0x00002,  "0"
HKR, ,                                  QoS,                            0x00002,  "0"
HKR, ,                                  rateCtrlEnable,                 0x00002,  "1"
HKR, ,                                  RTSThreshold,                   0x00002,  "2346"
HKR, ,                                  scanType,                       0x00002,  "2"
;HKR, ,                                  shortPreamble,                  0x00002,  "1"
;HKR, ,                                  sleepMode,                      0x00002,  "2"
HKR, ,                                  SwTxRetryScale,                 0x00002,  "6"
;HKR, ,                                  SmeEnable,                      0x00002,  "1"
;HKR, ,                                  tpc,                            0x00002,  "0"
HKR, ,					SSID,				0x00002,   "default"


HKR, CustomParams\Configurations,       MajorVersion,                   0x10003,  2
HKR, CustomParams\Configurations,       MinorVersion,                   0x10003,  0

HKR, CustomParams\Configurations,       SelectedConfigurationIndex,     0x10003,  0
HKR, CustomParams\Configurations,       SelectedConfigurationName,      0x00002,  "Default"


;-----------------------------------------------------------------------------
; A3AB NT specific
;

[A3AB.reg]
HKR, Ndi,             Service,      0, "A3AB"
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet"
HKR, ,                InitFile,     0, %InitFile%
HKR, ,                aifs,         0, "2"
HKR, ,                cwmin,        0, "15"


[A3AB.Service]
DisplayName     = %A3AB.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\A3AB.sys
LoadOrderGroup  = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, ,                  EventMessageFile,   0x00020000,   "%%SystemRoot%%\System32\netevent.dll"
HKR, ,                  TypesSupported,     0x00010001,   7

;----------------------------------------------------------------------------
; A3AB Win9x specific
;
[A3AB.win.reg]
HKR, ,                  DevLoader,          0,    "*ndis"
HKR, ,                  DeviceVxDs,         0,    "A3AB9x.sys"
HKR, ,                  EnumPropPages,      0,    "netdi.dll,EnumPropPages"

HKR, Ndi\Interfaces,    DefUpper,           0,    "ndis3"
HKR, Ndi\Interfaces,    DefLower,           0,    "ethernet"
HKR, Ndi\Interfaces,    UpperRange,         0,    "ndis3"
HKR, Ndi\Interfaces,    LowerRange,         0,    "ethernet"


HKR, NDIS,              LogDriverName,      0,    "A3AB9X"
HKR, NDIS,              MajorNdisVersion,   1,    03
HKR, NDIS,              MinorNdisVersion,   1,    0A
HKR, ,                  InitFile,           0,    %InitFile%
HKR, ,                  aifs,               0,    2
HKR, ,                  cwmin,              0,    15

HKR, Ndi\Install,       ndis3,              0,    "A3AB.install"

;-----------------------------------------------------------------------------
; DestinationDirs
;
[A3AB.win.CopyFiles]
A3AB9x.sys,,,2

[A3AB.CopyFiles.nt]
A3AB.sys,,,2

[CoInstallers_CopyFiles]
DWLInst.dll

[A3AB.DelIniFiles]
A3AB.ini,,,1

[Ndi_9X_CopyFiles]
DWLNdi.dll,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %A3AB_Disk%,,,

[SourceDisksFiles]
A3AB9x.sys	= 1,, ; on distribution disk 1
A3AB.sys		= 1,, ; on distribution disk 1
DWLNdi.dll	= 1,, ; on distribution disk 1
DWLInst.dll	 = 1,, ; on distribution disk 1

[DestinationDirs]
A3AB.CopyFiles.nt	= 12
A3AB.win.CopyFiles	= 10,system32\drivers ; %SystemRoot%\system32\drivers 
A3AB.DelIniFiles	= 10,system32\drivers ; %SystemRoot%\system32\drivers 
DefaultDestDir	 = 11
Ndi_9X_CopyFiles	 = 11

[DEFAULTDESTDIRS]
;


[Strings]
DLink			= "D-Link"
MapRegisters		= "Map Registers"
NetworkAddress		="Network Address"
sleepMode		= "Power Save Mode"
sleepModeOff                 = "CAM (Constantly Awake Mode)"
sleepModeNormal              = "Fast PSP (Power Save Mode)"
sleepModeMax                 = "Max PSP (Max Power Saving)"
tpc			= "Transmit Power"
tpcLowest		= "Lowest"
tpc12			= "12.5%"
tpc25			= "25%"
tpc50			= "50%"
tpc100			= "100%"
shortPreamble		= "802.11b Preamble"
shortPreambleEnable	= "Long and Short"
shortPreambleDisable	= "Long only"
radioEnable		= "Radio On/Off"
radioEnableOn		= "On"
radioEnableOff		= "Off"
InitFile		= "A3AB.ini"
A3AB_Disk		= "D-Link Wireless Driver Disk"
G650.DeviceDesc		= "D-Link AirPlus DWL-G650 Wireless Cardbus Adapter(rev.C)"
G520.DeviceDesc		= "D-Link AirPlus DWL-G520 Wireless PCI Adapter(rev.B)"
AG530.DeviceDesc	= "D-Link AirPremier DWL-AG530 Wireless PCI Adapter"
AG530B.DeviceDesc	= "D-Link AirPremier AG DWL-AG530 Wireless PCI Adapter"
AG660.DeviceDesc	= "D-Link AirPremier DWL-AG660 Wireless Cardbus Adapter"
AG660B.DeviceDesc	= "D-Link AirPremier AG DWL-AG660 Wireless Cardbus Adapter"
G510.DeviceDesc		= "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.B)"
G630.DeviceDesc         = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.D)"
G680.DeviceDesc		= "D-Link AirPremier DWL-G680 Wireless Cardbus Adapter"
G550.DeviceDesc		= "D-Link AirPremier DWL-G550 Wireless PCI Adapter"
G520P.DeviceDesc	= "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter"
G650P.DeviceDesc         = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter"
A3AB.Service.DispName	= "D-Link AirPro 802.11a/b Wireless Adapter Service(A3AB)"
